2021-2022 Results Summary Lead in Water Results School Name: Benjamin Franklin Middle School
Outlet Code
	
Sample ID
	
Location/Description
	Result (ppb)
	Above AL?

1WF
	
39-0505-BF01
	
WF outside the custodial area
	
ND
	
No

2WF
	
39-0505-BF02
	
WF in boy's locker room
	
ND
	
No

3WF
	
39-0505-BF03
	
WF in girl's locker room
	
ND
	
No

4BF
	
39-0505-BF04
	
WF/Filling Station across from Rm 112 (filler)
	
ND
	
No

5BB
	
39-0505-BF05
	WF/Filling Station across from Rm 112 (bubbler)
	
ND
	
No

6S
	
39-0505-BF06
	
Nurse office sink
	
ND
	
No

7BF
	
39-0505-BF07
	
WF/Filling Station next to Rm 107 (filler)
	
ND
	
No

8BB
	
39-0505-BF08
	
WF/Filling Station next to Rm 107 (bubbler)
	
2.64
	
No

9WF
	
39-0505-BF09
	
WF inside maintenance shop
	
2.63
	
No

10WF
	
39-0505-BF10
	
WF next to Rm 209
	
2.25
	
No

11WF
	
39-0505-BF11
	
WF at main office (left side)
	
ND
	
No

12WF
	
39-0505-BF12
	
WF at main office (right side)
	
ND
	
No

13WF
	
39-0505-BF13
	
WF next to Rm 203
	
ND
	
No

14WF
	
39-0505-BF14
	
WF/filler station inside cafeteria (filler)
	
ND
	
No

15WF
	
39-0505-BF15
	
WF/filler station inside cafeteria (bubbler)
	
ND
	
No

16WF
	
39-0505-BF16
	
WF inside cafeteria
	
ND
	
No

17WF
	
39-0505-BF17
	
WF across from Rm 308
	
ND
	
No

18WF
	
39-0505-BF18
	
WF next to Rm 304
	
ND
	
No

19WF
	
39-0505-BF19
	
WF in dance room
	
ND
	
No

BLANK
	
39-0505-BF20
	
Deionized Blank
	
ND
	
No

Action Level (AL) ≥15.5 parts per billion (ppb)

2021-2022 Results Summary Lead in Water Results School Name: Benjamin Franklin Middle School
Outlet Code
	
Sample ID
	
Location/Description
	Result (ppb)
	Above AL?

					

					

					

					

					

					

					

Action Level (AL) ≥15.5 parts per billion (ppb)

OrderID: 012207273

Page 1 Of	2

OrderID: 012207273

Page 2 Of	2

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone: (856) 303-2500	Fax: (856) 858-4571     Email: EnvChemistry2@emsl.com

Attn:	Tom Pruno	5/20/2022 Environmental Design, Inc.
5434 King Avenue Suite 101 Pennsauken, NJ 08109

Phone: (856) 616-9516 Fax:         (586) 616-9517

The following analytical report covers the analysis performed on samples submitted to EMSL Analytical, Inc. on 5/5/2022. The results are tabulated on the attached data pages for the following client designated project:

Teaneck Public Schools - Benjamin Franklin Middle School / Project #: PR-211214-1912

The reference number for these samples is EMSL Order #012207273. Please use this reference when calling about these samples. If you have any questions, please do not hesitate to contact me at (856) 303-2500.

Approved By:

Owen McKenna, Chemistry Laboratory Director

The test results contained within this report meet the requirements of NELAP and/or the specific certification program that is applicable, unless otherwise noted.

NELAP Certifications: NJ 03036, NY 10872, PA 68-00367, CA ELAP 1877

The samples associated with this report were received in good condition unless otherwise noted. This report relates only to those items tested as received by the laboratory. The QC data associated with the sample results meet the recovery and precision requirements established by the NELAP, unless specifically indicated. All results for soil samples are reported on a dry weight basis, unless otherwise noted. This report may not be reproduced except in full and without written approval by EMSL Analytical, Inc.

Page 1 of 6

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207273

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/5/2022 10:50 AM

Project: Teaneck Public Schools - Benjamin Franklin Middle School / Project #: PR-211214-1912

Client Sample Description	39-0505-BF01

WF Outside the Custodial Area

Analytical Results

Collected:

5/5/2022	Lab ID:	012207273-0001

5:56:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:27

Client Sample Description	39-0505-BF02

WF in Boy's Locker Room

Collected:	5/5/2022	Lab ID:	012207273-0002

5:58:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:31

Client Sample Description	39-0505-BF03

WF in Girl's Locker Room

Collected:	5/5/2022	Lab ID:	012207273-0003

5:59:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:33

Client Sample Description	39-0505-BF04

WF/Filling Station Across From Rm 112 (Filler)

Collected:	5/5/2022	Lab ID:	012207273-0004

6:01:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:34

Client Sample Description	39-0505-BF05

WF/Filling Station Across From Rm 112 (Bubbler)

Collected:	5/5/2022	Lab ID:	012207273-0005

5:52:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:39

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/20/2022 2:56:23 PM	Page 2 of 6

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207273

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/5/2022 10:50 AM

Project: Teaneck Public Schools - Benjamin Franklin Middle School / Project #: PR-211214-1912

Client Sample Description	39-0505-BF06

Nurse Office Sink

Analytical Results

Collected:

5/5/2022	Lab ID:	012207273-0006

5:57:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:41

Client Sample Description	39-0505-BF07

WF/Filling Station Across From Rm 107(Filler)

Collected:	5/5/2022	Lab ID:	012207273-0007

6:02:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:42

Client Sample Description	39-0505-BF08

WF/Filling Station Across From Rm 107 (Bubbler)

Collected:	5/5/2022	Lab ID:	012207273-0008

6:07:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

2.64	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:44

Client Sample Description	39-0505-BF09

WF Inside Maintenance Shop

Collected:	5/5/2022	Lab ID:	012207273-0009

6:04:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

2.63	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:45

Client Sample Description	39-0505-BF10

WF Next to Rm 209

Collected:	5/5/2022	Lab ID:	012207273-0010

6:06:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

2.25	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:47

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/20/2022 2:56:23 PM	Page 3 of 6

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207273

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/5/2022 10:50 AM

Project: Teaneck Public Schools - Benjamin Franklin Middle School / Project #: PR-211214-1912

Client Sample Description	39-0505-BF11

WF At Main Office (Left Side)

Analytical Results

Collected:

5/5/2022	Lab ID:	012207273-0011

6:08:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:48

Client Sample Description	39-0505-BF12

WF At Main Office (Right Side)

Collected:	5/5/2022	Lab ID:	012207273-0012

5:56:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:53

Client Sample Description	39-0505-BF13

WF/Filler Station Inside Cafeteria (Filler)

Collected:	5/5/2022	Lab ID:	012207273-0013

6:10:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:58

Client Sample Description	39-0505-BF14

WF/Filler Station Inside Cafeteria (Bubbler)

Collected:	5/5/2022	Lab ID:	012207273-0014

6:12:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:59

Client Sample Description	39-0505-BF15

WF Inside Cafeteria

Collected:	5/5/2022	Lab ID:	012207273-0015

6:12:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/19/2022	VD 00:01

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/20/2022 2:56:23 PM	Page 4 of 6

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207273

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/5/2022 10:50 AM

Project: Teaneck Public Schools - Benjamin Franklin Middle School / Project #: PR-211214-1912

Client Sample Description	39-0505-BF16

WF Across from Rm 308

Analytical Results

Collected:

5/5/2022	Lab ID:	012207273-0016

6:13:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/19/2022	VD 00:02

Client Sample Description	39-0505-BF17

WF Next to Rm 304

Collected:	5/5/2022	Lab ID:	012207273-0017

6:16:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/19/2022	VD 00:04

Client Sample Description	39-0505-BF18

WF in Dance Room

Collected:	5/5/2022	Lab ID:	012207273-0018

6:16:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/19/2022	VD 00:05

Client Sample Description	39-0505-BF19

Deionized Blank

Collected:	5/5/2022	Lab ID:	012207273-0019

6:23:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/19/2022	VD 00:07

Client Sample Description	39-0505-BF20	Collected:	5/5/2022	Lab ID:	012207273-0020 Trip Blank

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/19/2022	VD 00:08

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/20/2022 2:56:23 PM	Page 5 of 6

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207273

EDI50

Definitions:

MDL - method detection limit
J - Result was below the reporting limit, but at or above the MDL ND - indicates that the analyte was not detected at the reporting limit RL - Reporting Limit (Analytical)
D - Dilution Sample required a dilution which was used to calculate final results

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/20/2022 2:56:23 PM	Page 6 of 6