2021-2022 Results Summary Lead in Water Results School Name: Hawthorne Elementary School
Outlet Code
	
Sample ID
	
Location/Description
	Result (ppb)
	Above AL?

1WF
	
44-0505-HE01
	
WF next to Rm 43
	
3.54
	
No

3S
	
44-0505-HE02
	
Faculty Lounge sink
	
ND
	
No

4WF
	
44-0505-HE03
	
WF next to Rm 36
	
4.09
	
No

5WF
	
44-0505-HE04
	
WF across from Rm 33
	
3.8
	
No

7BF
	
44-0505-HE05
	
WF/Filler Station in cafeteria (filler)
	
ND
	
No

8BB
	
44-0505-HE06
	
WF/Filler Station in cafeteria (bubbler)
	
ND
	
No

9WF
	
44-0505-HE07
	
WF across from library
	
ND
	
No

10S
	
44-0505-HE08
	
Sink in library
	
1.05
	
No

BLANK
	
44-0505-HE09
	
Field Blank
	
ND
	
No

					

					

					

					

Action Level (AL) ≥15.5 parts per billion (ppb)

OrderID: 012207280

Page 1 Of	1

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone: (856) 303-2500	Fax: (856) 858-4571     Email: EnvChemistry2@emsl.com

Attn:	Tom Pruno	5/20/2022 Environmental Design, Inc.
5434 King Avenue Suite 101 Pennsauken, NJ 08109

Phone: (856) 616-9516 Fax:         (586) 616-9517

The following analytical report covers the analysis performed on samples submitted to EMSL Analytical, Inc. on 5/5/2022. The results are tabulated on the attached data pages for the following client designated project:

Teaneck Public Schools - Hawthorne Elementary School / Project #: PR-211214-1912

The reference number for these samples is EMSL Order #012207280. Please use this reference when calling about these samples. If you have any questions, please do not hesitate to contact me at (856) 303-2500.

Approved By:

Owen McKenna, Chemistry Laboratory Director

The test results contained within this report meet the requirements of NELAP and/or the specific certification program that is applicable, unless otherwise noted.

NELAP Certifications: NJ 03036, NY 10872, PA 68-00367, CA ELAP 1877

The samples associated with this report were received in good condition unless otherwise noted. This report relates only to those items tested as received by the laboratory. The QC data associated with the sample results meet the recovery and precision requirements established by the NELAP, unless specifically indicated. All results for soil samples are reported on a dry weight basis, unless otherwise noted. This report may not be reproduced except in full and without written approval by EMSL Analytical, Inc.

Page 1 of 3

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207280

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/5/2022 10:50 AM

Project: Teaneck Public Schools - Hawthorne Elementary School / Project #: PR-211214-1912

Client Sample Description	44-0505-H01

WF Next to Rm 43

Analytical Results

Collected:

5/5/2022	Lab ID:	012207280-0001

6:50:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

3.54	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:06

Client Sample Description	44-0505-H02

Faculty Lounge Sink

Collected:	5/5/2022	Lab ID:	012207280-0002

6:59:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:08

Client Sample Description	44-0505-H03

WF Next to Rm 36

Collected:	5/5/2022	Lab ID:	012207280-0003

7:00:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

4.09	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:10

Client Sample Description	44-0505-H04

WF Across From Rm 33

Collected:	5/5/2022	Lab ID:	012207280-0004

7:02:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

3.80	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:11

Client Sample Description	44-0505-H05

WF/Filler Station in Cafeteria (Filler)

Collected:	5/5/2022	Lab ID:	012207280-0005

7:04:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:13

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/20/2022 2:48:04 PM	Page 2 of 3

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207280

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/5/2022 10:50 AM

Project: Teaneck Public Schools - Hawthorne Elementary School / Project #: PR-211214-1912

Analytical Results

Client Sample Description	44-0505-H06

WF/Filler Station in Cafeteria (Bubbler)

Collected:	5/5/2022	Lab ID:	012207280-0006

7:05:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:14

Client Sample Description	44-0505-H07

WF Across From Library

Collected:	5/5/2022	Lab ID:	012207280-0007

7:08:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:16

Client Sample Description	44-0505-H08

Sink in Library

Collected:	5/5/2022	Lab ID:	012207280-0008

7:10:00 AM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

1.05	1.00 µg/L	5/17/2022	KG	5/18/2022	VD 23:20

Client Sample Description	44-0505-H09	Collected:	5/5/2022	Lab ID:	012207280-0009 Field Blank

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

Definitions:

5.43	1.00 µg/L	5/18/2022	VD	5/19/2022	VD 17:30

MDL - method detection limit
J - Result was below the reporting limit, but at or above the MDL ND - indicates that the analyte was not detected at the reporting limit RL - Reporting Limit (Analytical)
D - Dilution Sample required a dilution which was used to calculate final results

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/20/2022 2:48:04 PM	Page 3 of 3