2021-2022 Results Summary Lead in Water Results School Name: Whittier Elementary School
Outlet Code
	
Sample ID
	
Location/Description
	Result (ppb)
	Above AL?

1BF
	
39-0502-W01
	WF/ Filling Station next to Rm 129 (Nurse's Office) (filler)
	
ND
	
No

2BB
	
39-0502-W02
	WF/ Filling Station next to Rm 129 (Nurse's Office) (bubbler)
	
ND
	
No

3WF
	
39-0502-W03
	
WF next to Rm 124
	
1.56
	
No

4WF
	
39-0502-W04
	
WF next to Rm 102 & 103
	
2.17
	
No

5WF
	
39-0502-W05
	
WF next to Rm 108
	
1.82
	
No

6BF
	
39-0502-W06
	
WF/Filling Station (filler)
	
ND
	
No

7BB
	
39-0502-W07
	
WF/Filling Station (bubbler)
	
ND
	
No

8S
	
39-0502-W08
	
Cafeteria/Kitchen Sink (Rm 115)
	
ND
	
No

9S
	
39-0502-W09
	
WF next to Rm 216
	
ND
	
No

10WF
	
39-0502-W10
	
WF next to Rm 207
	
3.63
	
No

11WF
	
39-0502-W11
	
WF next to Rm 203
	
3.9
	
No

12WF
	
39-0502-W12
	
WF next to Rm 227
	
4.49
	
No

13WF
	
39-0502-W13
	
WF next to Rm 222
	
ND
	
No

BLANK
	
39-0502-W14
	
Field Blank
	
ND
	
No

					

					

Action Level (AL) ≥15.5 parts per billion (ppb)

OrderID: 012207104

Page 1 Of	2

OrderID: 012207104

Page 2 Of	2

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone: (856) 303-2500	Fax: (856) 858-4571     Email: EnvChemistry2@emsl.com

Attn:	Tom Pruno	5/19/2022 Environmental Design, Inc.
5434 King Avenue Suite 101 Pennsauken, NJ 08109

Phone: (856) 616-9516 Fax:         (586) 616-9517

The following analytical report covers the analysis performed on samples submitted to EMSL Analytical, Inc. on 5/3/2022. The results are tabulated on the attached data pages for the following client designated project:

Teaneck Public Schools - Whittier Elementary School / Project #: PR-211214-1912

The reference number for these samples is EMSL Order #012207104. Please use this reference when calling about these samples. If you have any questions, please do not hesitate to contact me at (856) 303-2500.

Approved By:

Owen McKenna, Chemistry Laboratory Director

The test results contained within this report meet the requirements of NELAP and/or the specific certification program that is applicable, unless otherwise noted.

NELAP Certifications: NJ 03036, NY 10872, PA 68-00367, CA ELAP 1877

The samples associated with this report were received in good condition unless otherwise noted. This report relates only to those items tested as received by the laboratory. The QC data associated with the sample results meet the recovery and precision requirements established by the NELAP, unless specifically indicated. All results for soil samples are reported on a dry weight basis, unless otherwise noted. This report may not be reproduced except in full and without written approval by EMSL Analytical, Inc.

Page 1 of 4

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207104

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/3/2022 12:50 PM

Project: Teaneck Public Schools - Whittier Elementary School / Project #: PR-211214-1912

Analytical Results

Client Sample Description	39-0502-W01

WF/ Filling Station Next to Rm 129 (Nurse's Office) (Filler)

Collected:	5/2/2022	Lab ID:	012207104-0001

12:18:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:19

Client Sample Description	39-0502-W02

WF/ Filling Station Next to Rm 129 (Nurse's Office) (Bubbler)

Collected:	5/2/2022	Lab ID:	012207104-0002

12:19:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:24

Client Sample Description	39-0502-W03

WF next to Rm 124

Collected:	5/2/2022	Lab ID:	012207104-0003

12:21:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

1.56	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:25

Client Sample Description	39-0502-W04

WF next to Rm 102 & 103

Collected:	5/2/2022	Lab ID:	012207104-0004

12:22:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

2.17	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:27

Client Sample Description	39-0502-W05

WF next to Rm 108

Collected:	5/2/2022	Lab ID:	012207104-0005

12:23:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

1.82	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:28

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/19/2022 10:18:49 AM	Page 2 of 4

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207104

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/3/2022 12:50 PM

Project: Teaneck Public Schools - Whittier Elementary School / Project #: PR-211214-1912

Client Sample Description	39-0502-W06

WF/Filling Station (Filler)

Analytical Results

Collected:

5/2/2022	Lab ID:	012207104-0006

12:24:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:33

Client Sample Description	39-0502-W07

WF/Filling Station (Bubbler)

Collected:	5/2/2022	Lab ID:	012207104-0007

12:25:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:35

Client Sample Description	39-0502-W08

Cafeteria/Kitchen Sink (Rm 115)

Collected:	5/2/2022	Lab ID:	012207104-0008

12:26:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:36

Client Sample Description	39-0502-W09

WF next to Rm 216

Collected:	5/2/2022	Lab ID:	012207104-0009

12:31:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:38

Client Sample Description	39-0502-W10

WF next to Rm 207

Collected:	5/2/2022	Lab ID:	012207104-0010

12:32:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

3.63	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:39

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/19/2022 10:18:49 AM	Page 3 of 4

EMSL Analytical, Inc.

200 Route 130 North, Cinnaminson, NJ 08077

Phone/Fax:	(856) 303-2500 / (856) 858-4571 http://www.EMSL.com                             EnvChemistry2@emsl.com

EMSL Order: CustomerID: CustomerPO:
ProjectID:

012207104

EDI50

Attn: Tom Pruno
Environmental Design, Inc. 5434 King Avenue
Suite 101 Pennsauken, NJ 08109

Phone: Fax:
Received:

(856) 616-9516 (586) 616-9517
5/3/2022 12:50 PM

Project: Teaneck Public Schools - Whittier Elementary School / Project #: PR-211214-1912

Client Sample Description	39-0502-W11

WF next to Rm 203

Analytical Results

Collected:

5/2/2022	Lab ID:	012207104-0011

12:34:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

3.90	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:41

Client Sample Description	39-0502-W12

WF next to Rm 227

Collected:	5/2/2022	Lab ID:	012207104-0012

12:35:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

4.49	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:46

Client Sample Description	39-0502-W13

WF next to Rm 222

Collected:	5/2/2022	Lab ID:	012207104-0013

12:37:00 PM

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:47

Client Sample Description	39-0502-W14	Collected:	5/2/2022	Lab ID:	012207104-0014 Field Blank

Prep Method	Parameter	Result	RL Units	Date & Analyst

Analysis Date & Analyst

METALS

200.8	Lead

Definitions:

ND	1.00 µg/L	5/16/2022	VD	5/17/2022	VD 11:52

MDL - method detection limit
J - Result was below the reporting limit, but at or above the MDL ND - indicates that the analyte was not detected at the reporting limit RL - Reporting Limit (Analytical)
D - Dilution Sample required a dilution which was used to calculate final results

ChemSmplw/RDL/NELAC-2.19.0.0 Printed: 5/19/2022 10:18:49 AM	Page 4 of 4